# Default to 921600 baud when flashing and monitoring device
CONFIG_ESPTOOLPY_BAUD_921600B=y
CONFIG_ESPTOOLPY_BAUD=921600
CONFIG_ESPTOOLPY_COMPRESSED=y
CONFIG_ESPTOOLPY_MONITOR_BAUD_115200B=y
CONFIG_ESPTOOLPY_MONITOR_BAUD=115200
CONFIG_ESPTOOLPY_FLASHSIZE_4MB=y

#enable BT
CONFIG_BT_ENABLED=y
CONFIG_BT_NIMBLE_ENABLED=y

#disable BT connection reattempt
CONFIG_BT_NIMBLE_ENABLE_CONN_REATTEMPT=n

#enable lwip ipv6 autoconfig
CONFIG_LWIP_IPV6_AUTOCONFIG=y

# Use a custom partition table
CONFIG_PARTITION_TABLE_CUSTOM=y
CONFIG_PARTITION_TABLE_FILENAME="partitions.csv"

# Disable chip shell
CONFIG_ENABLE_CHIP_SHELL=n

# Disable chip tests
CONFIG_BUILD_CHIP_TESTS=n

#enable lwIP route hooks
CONFIG_LWIP_HOOK_IP6_ROUTE_DEFAULT=y
CONFIG_LWIP_HOOK_ND6_GET_GW_DEFAULT=y

# External Platform
CONFIG_CHIP_ENABLE_EXTERNAL_PLATFORM=y
CONFIG_CHIP_EXTERNAL_PLATFORM_DIR="../../../../../builds/app-frameworks/platform/ESP32_custom"
CONFIG_CHIP_EXTERNAL_PLATFORM_INCLUDE_DIR="../../../../../builds/app-frameworks/"

# disable softap by default
CONFIG_ESP_WIFI_SOFTAP_SUPPORT=n

# Disable DS Peripheral
CONFIG_ESP_SECURE_CERT_DS_PERIPHERAL=n

# Enable HKDF in mbedtls
CONFIG_MBEDTLS_HKDF_C=y

# ESP32-DevKit Settings

