# Default to 921600 baud when flashing and monitoring device
CONFIG_ESPTOOLPY_BAUD_921600B=y
CONFIG_ESPTOOLPY_BAUD=921600
CONFIG_ESPTOOLPY_COMPRESSED=y
CONFIG_ESPTOOLPY_MONITOR_BAUD_115200B=y
CONFIG_ESPTOOLPY_MONITOR_BAUD=115200
CONFIG_ESPTOOLPY_FLASHSIZE_4MB=y

#enable BT
CONFIG_BT_ENABLED=y
CONFIG_BT_NIMBLE_ENABLED=y

#disable BT connection reattempt
CONFIG_BT_NIMBLE_ENABLE_CONN_REATTEMPT=n

#enable lwip ipv6 autoconfig
CONFIG_LWIP_IPV6_AUTOCONFIG=y

# Use a custom partition table
CONFIG_PARTITION_TABLE_CUSTOM=y
CONFIG_PARTITION_TABLE_FILENAME="partitions.csv"
CONFIG_PARTITION_TABLE_OFFSET=0xC000

# Enable chip shell
CONFIG_ENABLE_CHIP_SHELL=y

#enable lwIP route hooks
CONFIG_LWIP_HOOK_IP6_ROUTE_DEFAULT=y
CONFIG_LWIP_HOOK_ND6_GET_GW_DEFAULT=y

# Button
CONFIG_BUTTON_PERIOD_TIME_MS=20
CONFIG_BUTTON_LONG_PRESS_TIME_MS=5000

# disable softap by default
CONFIG_ESP_WIFI_SOFTAP_SUPPORT=n

# Disable DS Peripheral
CONFIG_ESP_SECURE_CERT_DS_PERIPHERAL=n

# Use compact attribute storage mode
CONFIG_ESP_MATTER_NVS_USE_COMPACT_ATTR_STORAGE=y

# Enable HKDF in mbedtls
CONFIG_MBEDTLS_HKDF_C=y

# Increase LwIP IPv6 address number to 6 (MAX_FABRIC + 1)
# unique local addresses for fabrics(MAX_FABRIC), a link local address(1)
CONFIG_LWIP_IPV6_NUM_ADDRESSES=6

# SPI Configuration
CONFIG_SPI_MASTER_ISR_IN_IRAM=n
CONFIG_SPI_SLAVE_ISR_IN_IRAM=n
CONFIG_HAL_SPI_MASTER_FUNC_IN_IRAM=n
CONFIG_HAL_SPI_SLAVE_FUNC_IN_IRAM=n

# ESP32-DFR0676 Settings
# Buttons
CONFIG_BSP_BUTTONS_NUM=1
CONFIG_BSP_BUTTON_1_TYPE_GPIO=y
CONFIG_BSP_BUTTON_1_GPIO=39
CONFIG_BSP_BUTTON_1_LEVEL=0
